ID programmer install manual

1. Hardware connect.

We have few kinds ID programmer for different products.

Now we using this ID programmer (photo shows) as example.



Insert the programmer USB port to PC USB PORT, and data line connect white box, the other USB mini port insert to watch charge PORT.

The watch and pager must power on then can be read and write.

The PC only can accept 1 PCS ID programmer, and run only 1 time ID software, Or maybe it cannot find ID programmer or find the wrong one.

1. Run the ID software. Different products, software maybe different.



If the read and write button is gray and not working, the most reason is not install driverproperly. The driver is under the ID dirtory /ID driver/setup.exe, run setup.exe. After install finished, read and write key will change to black color and working.

If not family the ID programming, you must first read then write, or the setting will be erase by default setting.